For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Lower Control Arm Screw Connections | 90 N·m | 67 lb ft
Plus 75 degrees plus 15 degrees
Lower Control Arm to Steering Knuckle Nuts | 50 N·m | 37 lb ft
Spring Strut Support Tube to Steering Knuckle

- Bolted Connections

50 N·m

37 lb ft

- Screwed Joint

85 N·m

62 lb ft

Plus 75 degrees plus 15 degrees
Steering Tie Rod End to Knuckle Nut | 30 N·m | 22 lb ft
Plus 90 degrees plus 15 degrees
Wheel Drive Shaft Boot Clamp | 25 N·m | 18 lb ft
Wheel Drive Shaft Nut

- First Pass

150 N·m

111 lb ft

- Second Pass

Loosen 45 degrees

- Third Pass - Tighten

250 N·m

185 lb ft