For 1990-2009 cars

#### Special Tools

KM-508-A /KM-508-A-2/KM-508-A-3 Control Arm Bushing Remover/Installer

### Removal Procedure

Important: In general, both damping bushings must be replaced in lower control arm.

1. Remove the lower control arm. Refer to Lower Control Arm Replacement .
2. Press the front damping bushing out with KM-508-A KM-508-A-1 (1) and (2).

### Installation Procedure

1. Coat the front damping bushing (1) and inside of tool KM-508-A and lower control arm with soap solution before pressing in.
2. Press in the front damping bushing with KM-508-A (3), KM-508-A (2) and KM-508-A (4).
3. Install the lower control arm. Refer to Lower Control Arm Replacement .