For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment sill trim plate.

• | Remove the liftgate weatherstrip.

• | Release the 8 clips (1, 2).

2. Remove the right-hand rear compartment side trim panel.

Release the 2 clips.

3. Release the servo motor.

• | Disconnect in the direction of the arrow.

• | Disconnect the wiring harness plug from the servo motor (1).

• | Release the wiring harness plug and disconnect.

4. Remove the cable for filler cap control.

• | Release the cable in the direction of the arrow.

• | Press the servo motor in the direction of the arrow and remove.

### Installation Procedure

1. Insert the servo motor.

• | Press in the direction of the tail lamp.

• | Connect and lock the wiring harness plug.

2. Install the cable for filler cap control and clip in.
3. Install the right side rear compartment side trim panel.

Fasten the 2 clips.

4. Install the rear compartment sill trim plate.

• | Install the 4 clips.

• | Install the liftgate weatherstrip.