For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat.

• | Disconnect at the loop (1) and support in the rear area, arrow.

• | Remove the rear seat upwards.

2. Remove the rear seat belt buckle.

• | Remove the bolt.

• | Remove the rear seat belt buckle.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

Note: Use screw locking compound.

1. Install the rear seat belt buckle.

Insert the rear seat belt buckle.

Tighten
Tighten the bolt to 20 N·m (15 lb ft).

2. Install the rear seat.

Insert the rear seat cushion and position.