For 1990-2009 cars

### Removal Procedure

1. Remove the ignition module. Refer to Ignition Coil Replacement .
2. Detach the engine management wiring harness from the intake manifold, cylinder head cover.

• | Disconnect the wiring harness (1) from the bracket.

• | Disconnect the wiring trough (2).

3. Remove the engine venting pipe (1).

• | Disconnect the wiring trough (2) from the cylinder head cover.

• | Disconnect the 2 quick-release fittings.

4. Remove the camshaft cover (1).

Remove the 11 bolts (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the camshaft cover.

Insert new gasket in the cylinder head cover.

Tighten
Tighten the 11 bolts to 8 N·m (71 lb in).

2. Install the engine venting pipe.

Connect the 2 quick-release fittings.

3. Attach the engine management wiring harness to the intake manifold.

• | Connect the wiring trough.

• | Clip the wiring harness into the guide.

4. Install the ignition module. Refer to Ignition Coil Replacement .