For 1990-2009 cars

#### Special Tools

KM6067 Radio Removal Tool

Important: When replacing the driver information display, before removing the control unit, carry out a Reset with the Tech 2. Refer to Control Module References.

### Removal Procedure

1. Disconnect the battery.

Important: Press the removal bars outwards and at the same time pull the radio out of bracket.

2. Remove the radio.

• | Insert the removal bars KM6067 into the mounting holes (arrows) and pull out the radio.

• | Disconnect the 2 wiring harness plugs (1, 2).

3. Remove the heating/air conditioning control. Refer to Heater and Air Conditioning Control Replacement.

• | Release the 2 clips (1).

• | Disconnect the 2 wiring harness plugs (2).

4. Remove the panel, instrument panel padding.

• | Remove the 2 bolts (1).

• | Disconnect the wiring harness plug (2).

5. Remove the information display.

• | Remove the 2 bolts (1).

• | Release and disconnect the wiring harness plug.

6. Remove the information display panel.

Release the 2 clips and remove upwards.

### Installation Procedure

1. Install the info display panel.

Install the 2 clips.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the information display.

Connect and latch the wiring harness plug.

Tighten
Tighten the 2 bolts to 2.5 N·m (22 lb in).

3. Install the panel, instrument panel padding.

• | Connect the wiring harness plug.

• | Install the 2 clips.

Tighten
Tighten the 2 bolts to 2.5 N·m (22 lb in).

4. Install the heating/air conditioning control. Refer to Heater and Air Conditioning Control Replacement.

• | Connect the 2 wiring harness plugs.

• | Install the 2 clips.

Important: The radio must engage audibly.

5. Install the radio.

Connect the 2 wiring harness plugs.

6. Connect the battery.
7. For programming procedures, refer to Control Module References.