For 1990-2009 cars

## Liftgate Wiring Harness Replacement Sedan

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect battery.
2. Remove the liftgate trim panel. Refer to Liftgate Trim Panel Replacement .
3. Remove the liftgate wiring harness.
4. Overview of the liftgate wiring harness.

Important: Cut through the clips with a suitable tool (flat screwdriver).

5. Disconnect the wiring harness to the left and right of the liftgate window.

Release the 4 clips.

### Installation Procedure

1. Install the liftgate wiring harness.
2. Install the liftgate trim panel. Refer to Liftgate Trim Panel Replacement .
3. Connect the battery.
4. For reprogramming procedures, refer to Control Module References .

## Liftgate Wiring Harness Replacement Coupe

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

Important: Replace or repair the wiring harnesses observing the safety regulations of electrics/electronics.

1. Disconnect the battery.
2. Remove the liftgate trim panel. Refer to Liftgate Trim Panel Replacement .
3. Remove the liftgate wiring harness.
4. Overview of liftgate wiring harness

### Installation Procedure

1. Install the liftgate wiring harness.
2. Install the liftgate trim panel. Refer to Liftgate Trim Panel Replacement .
3. Connect the battery.
4. For reprogramming procedures, refer to Control Module References .