For 1990-2009 cars

#### Special Tools

J 28733-B /KM-6610 and KM-956-1 Front/Rear Spindle Remover

### Removal Procedure

Caution: Refer to Brake Dust Caution in the Preface section.

Caution: Refer to Brake Fluid Irritant Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the front wheel. Refer to Tire and Wheel Removal and Installation .
3. Remove the brake disc. Refer to Front Disc Brake Pads Replacement .
4. Remove the nut from the axle shaft.

Counterhold against the wheel hub with the holding wrench J 28733-B /KM-6610 and KM-956-1 .

5. Disconnect the wiring harness plug (1) for the wheel sensor.

Important: Note the installation position of wheel bearing unit and cover plate.

6. Remove the wheel bearing unit.

• | Remove the 3 bolts (2).

• | Remove the wheel bearing unit (4) with the cover plate (3) from the steering knuckle and the axle shaft.

7. Remove the cover plate from the wheel bearing unit.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Important:

• | Note the installation position.

• | Clean the thread and insert the bolts with locking compound.

1. Install the wheel bearing unit.

• | Set the cover plate on the wheel bearing unit.

• | Push the wheel bearing unit with the cover plate on to the axle shaft and place on the steering knuckle.

• | Install 3 new wheel bearing unit bolts.

Tighten
Tighten the 3 new wheel bearing unit bolts to 90 N·m (66 lb ft), plus 30 degrees, plus 15 degrees.

2. Connect the wheel sensor wiring harness plug.
3. Install the axle shaft to the wheel hub with the new nut.

Tighten
Tighten the axle shaft wheel hub nut to 150 N·m (110 lb ft), undo 45 degrees, then tighten to 250 N·m (184 lb ft).

Counterhold with J 28733-B /KM-6610 and KM-956-1 .

4. Install the brake disc. Refer to Front Brake Rotor Replacement .
5. Lower the vehicle.
6. Install the front wheel. Refer to Tire and Wheel Removal and Installation .