For 1990-2009 cars

## Front Side Door Window Belt Inner Sealing Strip Replacement Sedan

### Removal Procedure

Caution: Refer to Express Down Feature Caution in the Preface section.

1. Lower the window.
2. Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the belt inner sealing strip.

Pull the sealing strip carefully from behind beginning at the top.

### Installation Procedure

1. Install the belt inner sealing strip.
2. Install the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Close the window.

## Front Side Door Window Belt Inner Sealing Strip Replacement Coupe

### Removal Procedure

Caution: Refer to Express Down Feature Caution in the Preface section.

1. Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the window belt inner sealing strip on inside of front door (2).

Remove the 5 retaining clamps (1).

### Installation Procedure

Important: Observe the installation position.

1. Install the window belt inner sealing strip on inside.

Install the 5 retaining clamps.

2. Install the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .