For 1990-2009 cars

### Removal Procedure

Warning: Refer to Hood Hold-Open Device Warning in the Preface section.

Caution: Refer to Liftgate Assist Rod Caution in the Preface section.

1. Open the hood.
2. Remove the strut.

2.1. | Support the hood.

2.2. | Open the 2 retaining clips.

2.3. | Remove the strut.

### Installation Procedure

1. Install the strut.
2. Install the strut support clip.
3. Close the hood.