For 1990-2009 cars

### Removal Procedure

Caution: Refer to Hood Hold-Open Device Caution in the Preface section.

Notice: Refer to Liftgate Assist Rod Notice in the Preface section.

1. Open the hood.
2. Remove the strut.

• | Support the hood.

• | Open the 2 retaining clips.

• | Remove the strut.

### Installation Procedure

1. Install the strut.
2. Install the strut support clip.
3. Close the hood.