For 1990-2009 cars

Table 1: | SDM Scan Tool Data Parameters
Table 2: | SDM Scan Tool Output Controls

#### SDM Scan Tool Data Parameters

Parameter | System State | Expected Value | Description
--- | --- | --- | ---
Operating Conditions: Ignition ON
AOS Status | -- | Empty Seat Supp. | The scan tool displays CS Suppression, Enabled, Suppressed or Empty Seat Supp. This is the current state of the automatic occupant sensor (AOS).
Driver Airbag Stage1 Squib Circuit Resistance | -- | Varies | This displays Ohms.
Driver Airbag Stage2 Squib Circuit Resistance | -- | Varies | This displays Ohms.
Driver Curtain Airbag Squib Circuit Resistance | -- | Varies | This displays Ohms.
Driver Pretensioner Squib Circuit Resistance | -- | Varies | This displays Ohms.
Driver Seat Position Sensor Status | -- | Varies | The scan tool displays Not Installed, Fault, Forward or Rearward.
Driver Seatbelt Status | -- | Not Buckled | The scan tool displays Buckled or Not Buckled. This is the current state of the driver seatbelt.
Driver Side Airbag Squib Circuit Resistance | -- | Varies | This displays Ohms.
Passenger Airbag Deactivation Status | -- | Varies | The scan tool displays Airbag On or Airbag Off. This is the state of the passenger airbag deactivation.
Passenger Airbag Stage1 Squib Circuit Resistance | -- | Varies | This displays Ohms.
Passenger Airbag Stage2 Squib Circuit Resistance | -- | Varies | This displays Ohms.
Passenger Curtain Airbag Squib Circuit Resistance | -- | Varies | This displays Ohms.
Passenger Pretensioner Squib Circuit Resistance | -- | Varies | This displays Ohms.
Passenger Seat Position Sensor Status | -- | Varies | The scan tool displays Not Installed, Fault, Forward or Rearward.
Passenger Seatbelt Status | -- | Not Buckled | The scan tool displays Buckled or Not Buckled. This is the state of the passenger seatbelt.
Passenger Side Airbag Squib Circuit Resistance | -- | Varies | This displays Ohms.

#### SDM Scan Tool Output Controls

Output Control | Description
--- | ---
Clear Deployment Record | This output control is used to clear the airbag deployment record.
Read ECU Identification | This output control is used to read the electronic control unit (ECU) or control module identification data.
Program ECU | This output control is used to program the electronic control unit (ECU) or control module.
Program Low Speed CAN-Bus Config. | This output control is used to program the low speed control area network (CAN) serial data bus configuration.
Program Seat Belt Reminder | This output control is used to program the seat belt reminder.
Read Variant Configuration | This output control is used to read the variant configuration.
Seat Belt Reminder Data | This output control is used to view the seat belt reminder data.