For 1990-2009 cars

### Removal Procedure

1. Remove the corresponding outer tie rod end from the tie rod. Refer to Steering Linkage Outer Tie Rod Replacement.

Note: To remove and refit the right-hand tie rod the left-hand boot must also be detached from the steering gear. A flat surface is to be found on the steering shaft side to hold against the steering rack (arrows).

2. Remove the corresponding boot. Refer to Rack and Pinion Boot Replacement.
3. Remove the inner tie rod from the steering rack.

Counterhold with an open-ended wrench (2) on the toothed rack flat.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the tie rod inner linkage to the steering gear.

Tighten
Tighten to 90 N·m (67 lb ft).

• | Clean the rack thread and coat with locking compound.

• | Install the inner tie rod to the rack.

| Counterhold with an open-ended wrench (2) on the toothed rack flat (arrow).

2. Install the boot or boots. Refer to Rack and Pinion Boot Replacement.
3. Install the corresponding outer tie rod end. Refer to Steering Linkage Outer Tie Rod Replacement.
4. Check the straight-ahead position, adjust if necessary. Refer to Straight Ahead Inspection.
5. Check the toe-in, adjust if necessary. Refer to Wheel Alignment - Steering Wheel Angle and/or Front Toe Adjustment.