For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Bag Control Unit Nuts | 10 N·m | 89 lb in
Assist Handle Bolts | 2.8 N·m | 23 lb in
Cable Harness Clamp Nut | 5 N·m | 44 lb in
Center Pillar Bolt - Lower | 35 N·m | 26 lb ft
Center Pillar Bolt - Upper | 2.5 N·m | 22 lb in
Diagnostics Plug Bracket Nuts | 10 N·m | 89 lb in
Front Seat Bolts - Driver Side | 35 N·m | 26 lb ft
Front Seat Belt to Front Seat Bolts - Left and Right | 20 N·m | 15 lb ft
Front Seat Bolts - Passenger Side | 35 N·m | 26 lb ft
Front Seat Guide Bolt - Passenger Side | 35 N·m | 26 lb ft
Ground Strap Nut | 5 N·m | 44 lb in
Instrument Panel Padding Bracket Bolts | 13 N·m | 113 lb in
Instrument Panel Padding Retainer Bolts | 13 N·m | 113 lb in
Interior Light Bolts | 1.5 N·m | 13 lb in
Interior Light Bracket Bolts - Front | 1.5 N·m | 13 lb in
Rear Seat Backrest Bolt | 40 N·m | 30 lb ft
Rear Seat Backrest Guide Bolts | 20 N·m | 15 lb ft
Rear Seat Backrest to Seat Belt Buckle Bolts | 20 N·m | 15 lb ft
Roof Rail Stowage Compartment Bolts | 2.8 N·m | 23 lb in
Seat Belt Bolt | 35 N·m | 26 lb ft
Seat Belt Bolt - Left Side | 20 N·m | 15 lb ft
Seat Belt Bolt - Right Side | 20 N·m | 15 lb ft
Seat Belt Bolt - Left and Right Upper Center Pillar Trim | 35 N·m | 26 lb ft
Seat Belt Striker Bolt - Lower | 35 N·m | 26 lb ft
Seat Belt to Center Pillar Bolt | 35 N·m | 26 lb ft
Shifter Rod Bolt

- First Pass

12 N·m

106 lb in

- Final Pass

Plus 180-225 Degrees

Sunshade Bolts - Left and Right | 2.2 N·m | 19 lb in
Sunshade Main Bracket Bolts | 1.5 N·m | 13 lb in
Yaw Sensor Nuts | 6 N·m | 53 lb in