For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

Important: Wait 1 minute for the airbag to deactivate.

1. Disconnect the battery.
2. Remove the front seat belt securing the panel (1).
3. Remove the seat belt from the front seat.

Remove the bolt (2).

4. Position the seat to the most forward position.
5. Remove the drivers seat, rear.

Remove the 2 bolts (1).

Important: Disconnect the wiring harness plug.

6. Remove the front seat.

Remove from the front guide.

7. Remove the height adjuster panel.

Release with a plastic wedge.

8. Remove the height adjuster.
9. Remove the 2 bolts (1) and the lever.
10. Remove the adjuster wheel, seat backrest.

Release with a plastic wedge.

11. Remove the outer paneling.

• | Remove the 2 bolts (1, 3).

• | Remove the front of paneling from the guide (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the exterior paneling.

Insert the paneling.

Tighten
Tighten the 2 bolts to 35 N·m (26 lb ft).

2. Install the adjuster wheel, seat backrest.

Install the adjusting wheel.

3. Install the height adjuster.

Tighten
Tighten the 2 bolts to 35 N·m (26 lb ft).

4. Install the height adjuster panel.

Install the panel.

Important: Connect the wiring harness plug.

5. Install the front seat.

Insert into the front guide.

6. Install the front seat, rear.

Tighten
Tighten the 2 bolts to 35 N·m (26 lb ft).

7. Reposition the seat to the original position.
8. Install the seat belt at the front seat.

Tighten
Tighten the bolt to 20 N·m (15 lb ft).

9. Install the seat belt fastening panel.
10. Connect the battery.
11. For programming procedures, refer to Control Module References .