For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

Important: Wait 1 minute for airbag to deactivate.

1. Disconnect the battery.
2. Remove the front seat belt securing the panel (1).
3. Remove the seat belt from the front seat.

Remove the bolt (2).

4. Place the seat in the most forward position.
5. Remove the rear drivers seat.

Remove the 2 bolts (1).

Important: Disconnect the wiring harness plug.

6. Remove the front seat.

Remove from the front guide.

7. Remove the interior paneling.

• | Remove the bolt (1).

• | Remove the paneling.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the interior paneling.

Insert the paneling.

Tighten
Tighten the bolt to 2.5 N·m (22 lb in).

Important: Connect the wiring harness plug.

2. Install the front seat.

Insert into the front guide.

3. Install the front seat, rear.

Tighten
Tighten the 2 bolt to 35 N·m (26 lb ft).

4. Reposition the seat to the original position.
5. Install the seat belt at the front seat.

Tighten
Tighten the bolt to 20 N·m (15 lb ft).

6. Install the seat belt fastening panel.
7. Connect the battery.
8. For programming procedures, refer to Control Module References .