For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Axle Shaft Nut

- First Pass

150 N·m

111 lb ft

- Second Pass

Undo 45 Degrees

- Third Pass

250 N·m

185 lb ft

Engine Compartment Cover Bolts - Left and Right | 5 N·m | 44 lb in
Engine Compartment Cover Bolts - Lower | 5 N·m | 44 lb in
Engine Support Bolt - Lower Rear | 80 N·m | 59 lb ft
Front Axle Housing Bolts | 90 N·m | 67 lb ft
Plus 45 Degrees Plus 15 Degrees
Front Wheel Bolts | 110 N·m | 81 lb ft
Intermediate Shaft Clamping Screw | 24 N·m | 17 lb ft
Lower Control Arm Front Frame Screw | 90 N·m | 67 lb ft
Plus 75 Degrees Plus 15 Degrees
Lower Control Arm Screw Connections | 90 N·m | 67 lb ft
Plus 75 Degrees Plus 15 Degrees
Lower Control Arm to Steering Knuckle Nuts | 50 N·m | 37 lb ft
Rubber Insulator Bolts | 20 N·m | 15 lb ft
Rubber Insulator Shell Bolt | 20 N·m | 15 lb ft
Spring Strut Support Tube to Steering Knuckle

- Bolted Connections

50 N·m

37 lb ft

- Screwed Joint

85 N·m

62 lb ft

Plus 75 Degrees Plus 15 Degrees
Stabilizer Retaining Bracket Bolts | 20 N·m | 15 lb ft
Stabilizer Shaft Link Nuts | 65 N·m | 48 lb ft
Stabilizer Shaft Link Bolt | 55 N·m | 40 lb ft
Sump Bracket Bolts | 25 N·m | 18 lb ft
Triangular Support to Vehicle Underbody Bolt | 65 N·m | 48 lb ft
Wheel Bearing Unit Bolts | 90 N·m | 67 lb ft
Plus 30 Degrees Plus 15 Degrees