For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery.
2. Wait 1 minute for the airbag to deactivate.
3. Remove the resonator.

• | Remove the bolt (2).

• | Remove the resonator (1) from the guide (arrow).

4. Remove the airbag sensor.

• | Remove the 2 bolts (1).

• | Disconnect the wiring harness plug and remove the sensor.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the airbag sensor.

Insert the sensor and connect the wiring harness plug.

Tighten
Tighten the 2 bolts to 6 N·m (53 lb in).

2. Install the resonator.

Insert the resonator into the guide.

Tighten
Tighten the bolt to 2.5 N·m (22 lb in).

3. Connect the battery.

Tighten
Tighten the bolt to 5 N·m (44 lb in).

4. Perform the readiness inspection.
5. For programming procedures, refer to Control Module References.