For 1990-2009 cars

### Removal Procedure

1. Remove the upper extension trim.

• | Release the panel with a plastic wedge.

• | Release the 3 clips.

Important: Only for electrically operated outer mirror.

2. Disconnect the wiring harness plug.

### Installation Procedure

1. Install the upper extension trim.

Important: Only for electrically operated outer mirror.

2. Connect the wiring harness plug.

Install the 3 clips.