For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Alternator Bolts | 35 N·m | 26 lb ft
Alternator Wiring Harness Nuts | 7 N·m | 67 lb in
Bearing Support to End Shield with Pawl Bolts | 9 N·m | 80 lb in
Bearing Support with Rocker Arm in End Shield | 22 N·m | 16 lb ft
Bracket to the Cylinder Block Bolts | 20 N·m | 15 lb ft
Bridge Bolts | 7 N·m | 62 lb in
Central Release Bolts | 5 N·m | 44 lb in
Compressor Bolts | 22 N·m | 16 lb ft
Coolant Pipe to the Coolant Module Bolts | 25 N·m | 18 lb ft
Coolant Pipe to the Oil Filter Housing Bolt | 25 N·m | 18 lb ft
Coolant Pipe, Oil Filter Housing to the Thermostat Housing Bolts | 8 N·m | 71 lb ft
Differential Bearing Ring Retaining Plate to Transmission Housing Bolt | 9 N·m | 80 lb in
Differential Ring Gear to Differential Housing Bolts

- 1st Pass

70 N·m

52 lb ft

- 2nd Pass

30 degrees

- 3rd Pass

15 degrees

Dipstick Guide Tube Bolt | 8 N·m | 71 lb ft
End Shield to Transmission Housing Bolts | 22 N·m | 16 lb ft
End Shield Cover To Transmission Housing, with new gasket

- M7 Bolts (Qty: 4)

15N·m

11 lb in

- M8 Bolts (Qty: 5)

20 N·m

15 lb ft

End Shield Cover To Transmission Housing, plastic cover with integral seal

- M6 Bolts (Qty: 4)

8 N·m

71 lb in

- M8 Bolts (Qty: 5)

20 N·m

15 lb ft

Exhaust Manifold with the Catalytic Converter Nuts | 20 N·m | 15 lb ft
Fluid Inspection Bolt

- 1st Pass

4 N·m

35 lb ft

- 2nd Pass

45-135 degrees

Front Engine Damping Block Bracket Bolt | 80 N·m | 59 lb ft
Front Engine Damping Block Screwed Joint to Front Axle Body | 55 N·m | 41 lb ft
Gearbox Cover to Transmission Bolts | 15 N·m | 11 lb ft
Gearshift Rod Bolt

- 1st Pass

12 N·m

106 lb in

- 2nd Pass

180-225 degrees

Oil Pan to Transmission Bolts | 40 N·m | 30 lb ft
Pressure Line Retaining Nut | 14 N·m | 10 lb ft
Rear Engine Damping Block Screwed Joint to Front Axle Body | 55 N·m | 41 lb ft
Reversing Lamp Switch | 20 N·m | 15 lb ft
Transmission to Cylinder Block Bolts | 60 N·m | 44 lb ft
Upper Engine Cover Bolts | 7 N·m | 62 lb in
Wiring Harness Bracket Bolts, Transmission to Cylinder Block | 60 N·m | 44 lb ft
Wiring Harness Bracket Bolts, Transmission to Oil Pan | 40N·m | 30 lb ft