For 1990-2009 cars

### Removal Procedure

1. Remove the front of the rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement.
2. Remove the rear quarter speaker.

• | Remove the 3 bolts (1).

• | Disconnect the wiring harness plug (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the rear quarter speaker.

Connect the wiring harness plug.

Tighten
Tighten the 3 bolts to 2.5 N·m (22 lb in).

2. Install the front inner paneling of the rear quarter panel. Refer to Quarter Lower Rear Trim Panel Replacement.