For 1990-2009 cars

#### Special Tools

KM-652 Flywheel Holding Tool

### Removal Procedure

1. Remove the manual transmission. Refer to Transmission Replacement .
2. Remove the thrust plate and clutch disc. Refer to Clutch, Pressure Plate, and Pilot Bearing Replacement .
3. Remove the flywheel.

• | Lock the flywheel via the starter ring gear with KM-652 (1).

• | Remove the 6 bolts.

### Installation Procedure

1. Install the flywheel.

• | Clean the thread in the crankshaft.

Notice: Refer to Fastener Notice in the Preface section.

• | Use new bolts.

Tighten
Tighten the 6 bolts to 35 N·m (26 lb ft) plus 30 degrees plus 15 degrees.

• | Remove KM-652 .

2. Install the thrust plate and clutch disc. Refer to Clutch, Pressure Plate, and Pilot Bearing Replacement .
3. Install the manual transmission. Refer to Transmission Replacement .