For 1990-2009 cars

### Removal Procedure

1. Remove the front seat back covering. Refer to Front Seat Back Cushion Cover Replacement .
2. Remove the active head restraint frame.

• | Detach the active head restraint tension spring.

• | Remove the 2 bolts (l).

• | Remove frame from guide (arrows).

3. Undo the 2 mounting bearings of the active head restraint.

### Installation Procedure

1. Install the 2 mounting bearings of the active head restraint.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the active head restraint frame.

• | Insert the frame.

Tighten
Tighten the 2 bolts to 3.5 N·m (32 lb in).

• | Attach the active head restraint tension spring.

3. Attach the front seat back covering. Refer to Front Seat Back Cushion Cover Replacement .