For 1990-2009 cars

### Removal Procedure

1. Remove the battery. Refer to Battery Replacement .
2. Place the drain pan below the surge tank.
3. Remove the surge tank.

• | Unclip the coolant hoses.

• | Detach the coolant hoses (1).

### Installation Procedure

1. Install the surge tank.

Attach the coolant hoses.

2. Install the battery. Refer to Battery Replacement .
3. Fill the cooling system. Refer to Cooling System Draining and Filling .