For 1990-2009 cars

### Removal Procedure

1. Remove the wire harness connector from the clutch pedal engine start switch.
2. Remove the switch from the instrument panel (I/P).

### Installation Procedure

1. Install the clutch pedal engine start switch to the I/P.
2. Install the wire harness connector to the switch.
3. Verify proper operation of the switch.

The starter should engage only when the clutch is fully disengaged.