For 1990-2009 cars

### Removal Procedure

Caution: Striker alignment is a crucial part of door latch operation. Do not use the door striker to adjust the door to the vehicle. Failure to properly adjust the striker can result in damage to the door latch and the striker.

1. Open the rear door.

Note: Mark the previous installation position.

2. Remove the rear door lock striker (1).

Remove the 2 bolts (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the rear door lock striker.

Tighten
Tighten the 2 bolts to 20 N·m (15 lb ft).

2. Close the rear door.