For 1990-2009 cars

#### Special Tools

KM-962-A /KM-962-10 Tester

### Removal Procedure

1. Remove the battery.

• | Disconnect the negative cable (2) from the battery.

| Remove the nut.

• | Disconnect the positive cable (3) from the battery.

| Remove the nut.

• | Remove the bracket (1).

| Remove the bolt (4).

• | Remove the battery.

2. Remove the battery support.

• | Release the cable tie.

• | Remove the 3 bolts (1).

3. Connect KM-962-A (3) to the wiring harness plug of the selector lever position switch

• | Disconnect the wiring harness plug of the selector lever position switch (1).

• | Open the locking shackle.

4. Connect KM-962-A with KM-962-A KM-962-10 (2) to the battery.
5. Inspect the setting of the selector lever position switch.

| Note: The light diodes corresponding to the markings on the insert module (1) must flash for each individual gear.

• | Shift through all the gears one after the other.

• | If the setting is incorrect:

- | Adjust the selector cable. Refer to Range Selector Lever Cable Adjustment.

- | Adjust the selector lever position switch. Refer to Transmission Range Switch Adjustment.

- | Inspect the electrical function of the selector lever position switch.

- | See test instructions.

### Installation Procedure

1. Connect the selector lever position switch wiring harness plug.

• | Disconnect KM-962-A from the selector lever position switch wiring harness plug.

• | Disconnect KM-962-A from KM-962-10.

• | Disconnect KM-962-A from the battery.

• | Lock the wiring harness plug.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the battery support.

Fasten the cable tie.

Tighten
Tighten 3 bolts 10 N·m (89 lb in).

3. Install the battery.

• | Install the bracket (1).

• | Tighten the bolt (4).

Tighten
Tighten bolt 15 N·m (11 lb ft).

• | Connect the positive cable (3) to the battery.

• | Connect the negative cable (2) to the battery.

4. For programming procedures, refer to Control Module References.