For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console. Refer to Front Floor Console Replacement.
2. Remove the range selector cable (2) from the selector lever.

• | Remove the retaining clamp (1).

• | Disconnect the selector lever cable from the bracket.

3. Remove the range selector lever assembly.

• | Disconnect the wiring harness plug (1).

• | Remove the 4 bolts (2).

• | Remove the selector lever assembly.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the selector lever assembly.

• | Insert the range selector lever assembly.

Tighten
Tighten the 4 bolts to 5 N·m (44 lb in).

• | Connect the wiring harness plug (1).

2. Install the selector cable (2) to the selector lever.

• | Install the selector lever cable to the bracket.

• | Install the retaining clamp.

3. Install the front floor console. Refer to Front Floor Console Replacement.
4. For programming procedures, refer to Control Module References.