For 1990-2009 cars

## Liftgate Emblem/Nameplate Replacement Sedan

### Removal Procedure

Important: Do not heat the chrome coating to more than 90°C (194°F) as there is a risk of damage. Put the heat gun on its lowest setting and maintain a sufficient distance.

1. Heat the lettering with a heat gun and pull off the backing.

Important: Clean with cleaners naphtha or silicone remover.

2. Clean the surface to be bonded.

### Installation Procedure

Important: Install the emblem/nameplate in the center.

Position the lettering in accordance with the dimensional data and stick on.

#### Saturn Emblem

Height above trim strip to lower edge of the logo (I), 68 mm (2.7 in).

#### Astra Lettering Left

• | Distance from upper edge of strip to the lower edge of lettering (IV), 38 mm (1.5 in).

• | Distance from left of the lettering to the lower corner of the strip (V), 30 mm (1.2 in).

#### Engine Designation on the Right

• | Distance from upper edge of strip to lower edge of lettering (II), 38 mm (1.5 in).

• | Distance from the right of the lettering the lower right corner of the strip (III), 33 mm (1.3 in).