For 1990-2009 cars

### Removal Procedure

1. Open the instrument panel (I/P) compartment.
2. Remove the I/P compartment lamp.

• | Disconnect the lamp (1).

• | Disconnect the wiring harness plug (2).

• | Remove the lamp.

### Installation Procedure

1. Install the I/P compartment lamp.

• | Install the lamp.

• | Connect the wiring harness plug.

• | Install the I/P compartment lamp.

2. Close the I/P compartment.