For 1990-2009 cars

### Removal Procedure

1. Remove the radio.

1.1. | Disconnect with the dismantling strap, arrow.

1.2. | Disconnect the wiring harness plug (2).

1.3. | Disconnect the antenna (1).

2. Remove the heating/air conditioning control module.

2.1. | Loosen the 2 top clips (1).

2.2. | Loosen the 2 bottom clips.

2.3. | Release the 2 wiring harness plugs and disconnect (2).

3. Remove the instrument panel (I/P) center trim panel.

3.1. | Remove the 2 bolts (2).

3.2. | Release and disconnect the wiring harness plug (1).

3.3. | Remove the center trim panel.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the center trim panel.

Connect and latch the wiring harness plug.

Tighten
Tighten the 2 bolts to 2.5 N·m (22 lb in).

2. Install the heating/air conditioning control module.

2.1. | Connect and lock the 2 wiring harness plugs.

2.2. | Install the 4 clips.

3. Install the radio.

3.1. | Install the antenna.

3.2. | Connect the wiring harness plug.

3.3. | Slide the radio in until it clicks in.