For 1990-2009 cars

### Removal Procedure

1. Remove the bench seat.

• | Unlock 2 brackets (1) front.

• | Support the 2 bench seats from the rear bracket.

• | Push the seat simultaneously backwards and upward.

2. Remove the cushion cover clamp.

Remove the 48 clamps.

3. Loosen the surrounding upholstery.
4. Remove the cushion cover clamps from the seat area.

• | Remove the 21 clamps.

• | Remove the cushion cover covering.

### Installation Procedure

1. Fasten the rear seat cushion cover on the seat area.

• | Position upholstery covering.

• | Install the 21 clamps.

2. Place the cushion cover all the way around.
3. Install the cushion cover clamps.

Install the 48 clamps.

4. Install the rear seat.

Insert the rear seat cushion and position.