For 1990-2009 cars

#### Special Tools

KM-907 Control Arm Bushing Remover/Installer

### Removal Procedure

Important: Damping bushings in the front frame must always be replaced in pairs.

1. Remove the front frame. Refer to Front Frame Replacement .
2. Press the corresponding damping bushing (4) out of the front frame with the KM-907-11 (3), KM-907-12 (1) and KM-907-30 (2).

### Installation Procedure

1. Install the new damping bushings in the front frame.

• | Coat the damping bushings and guide in the front axle body with soapy solution.

• | Draw the corresponding damping bushing (3) into the front frame with the KM-907-13 (2), KM-907-14 (1) and KM-907-30.

2. Install the front frame. Refer to Front Frame Replacement .