For 1990-2009 cars

### Removal Procedure

1. Remove the upholstery covering all the way around.
2. Remove the head restraint guide sleeve.

Remove the 2 head restraint guide sleeves with the appropriate tool.

3. Remove the upholstery covering.

Remove the 7 clamps.

Remove the upholstery covering.

### Installation Procedure

1. Install the upholstery covering.

Position the upholstery covering.

Install the 7 clamps.

2. Install the head restraint guide sleeve.

Engage the 2 head restraint guide sleeves (audible click).

3. Insert the surrounding upholstery covering.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the left bracket.

Tighten
Tighten the bolt to 25 N·m (18 lb ft).

5. Install the right bracket.

Tighten
Tighten the 2 bolts to 25 N·m (18 lb ft).

6. Install the rear seat back cushion cover.

Install the 9 clips.

7. Install the headrest.
8. Insert the rear seat back cushion.
9. Install the rear seat back cushion.

Tighten

• | Tighten the 2 bolts, side to 20 N·m (15 lb ft).

• | Tighten the screw at back to 20 N·m (15 lb ft).

Important: Use screw locking compound.

10. Fold down the rear seat back cushion.

Insert the seat belt buckle.

Tighten
Tighten the front screw to 20 N·m (15 lb ft).

11. Install the rear seat.

Insert the rear seat cushion and position.