For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the camshaft position sensor of the intake camshaft (2).

• | Disconnect the wiring harness plug (1).

• | Remove the bolt.

3. Remove the camshaft position sensor of the exhaust camshaft (4).

• | Disconnect the wiring harness connector (3).

• | Disconnect the wiring harness of the oxygen sensor from the bracket.

• | Remove the bolt.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the camshaft position sensor of the exhaust camshaft.

Tighten
Tighten the bolt to 6 N·m (53 lb in).

• | Connect the wiring harness of the oxygen sensor to the bracket.

• | Install the wiring harness plug.

2. Install the camshaft position sensor, intake camshaft.

Tighten
Tighten the bolt to 6 N·m (53 lb in).

3. Connect the wiring harness plug.
4. Close the hood.