For 1990-2009 cars

## Front Side Door Check Link Replacement Sedan

### Removal Procedure

1. Remove the front door side panel. Refer to Front Side Door Trim Panel Replacement .
2. Partially loosen the water vapor barrier (1).

Remove the 2 clips (2).

3. Remove the check link (2).

• | Remove the bolt (1).

• | Remove the 2 nuts (3).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install check link.

Tighten

• | Tighten the 2 nuts to 8 N·m (71 lb in).

• | Tighten the bolt to 20 N·m (15 lb ft).

2. Install the water vapor barrier.

Install the 4 clips.

3. Install the front side door trim panel. Refer to Front Side Door Trim Panel Replacement

## Front Side Door Check Link Replacement Coupe

### Removal Procedure

1. Remove the front side door check link from the A-pillar.

Remove the bolt (1).

2. Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Partially loosen the water vapor barrier (1).

• | Remove the external mirror wiring harness.

• | Remove the 2 cable brackets (2).

4. Remove the check link.

Remove the 2 nuts (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the check link.

Tighten
Tighten the 2 nuts to 8 N·m (71 lb in).

2. Install the water vapor barrier.

• | Install the external mirror wiring harness.

• | Replace the 2 cable brackets.

3. Install the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .
4. Install the check link to the A-pillar.

Tighten
Tighten the bolt to 20 N·m (15 lb ft).