For 1990-2009 cars

### Removal Procedure

Remove the backup lamp switch (1).

• | Disconnect the wiring harness plug from the backup lamp switch.

• | Remove the backup lamp switch.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Important: Use a new seal ring.

1. Install the backup lamp switch.

• | Tighten the backup lamp switch (1).

Tighten
Tighten to 20 N·m (15 lb ft).

• | Connect the wiring harness plug to the backup lamp switch.

2. Inspect the transmission fluid level. Refer to Transmission Fluid Check .