For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console. Refer to Front Floor Console Replacement .
2. Remove the selector linkage (2) from the selector lever.

• | Remove the retaining clamp (1).

• | Disconnect the selector lever from the bracket.

3. Remove the selector lever assembly.

• | Disconnect the wiring harness plug (1).

• | Remove the 4 bolts (2).

• | Remove the selector lever assembly.

4. Remove the lock control solenoid selector lever lock (2).

| Important: Note the configuration of cables.

• | Disconnect the 2 wiring plugs (1) from the lock control solenoid.

• | Remove the 2 bolts (3).

• | Remove the lock control solenoid from the selector lever lock.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Important: Note the configuration of cables.

1. Install the lock control solenoid for the selector lever lock (2).

• | Insert the lock control solenoid for the selector lever lock.

Tighten
Tighten the 2 bolts (3) to 4 N·m (35 lb in).

• | Connect the 2 wiring plugs (1) to the lock control solenoid.

2. Install the selector lever assembly.

• | Insert the selector lever assembly.

Tighten
Tighten 4 bolts (2) 5 N·m (44 lb in).

• | Connect the wiring harness plug (1).

3. Install the selector linkage (2) to the selector lever.

• | Install the selector lever to the bracket.

• | Install the retaining clamp (1).

4. Install the front floor console. Refer to Front Floor Console Replacement .
5. Check the selector lever safety functions.
6. For reprogramming procedures, refer to Control Module References .