For 1990-2009 cars

#### Special Tools

KM-6009 Remover/Installer

1. Insert a NEW gasket in the camshaft head cover.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the camshaft cover (1) and bolts (2).

Tighten
Tighten the 11 bolts to 8 N·m (71 lb in).

3. Install the engine venting pipe (1).
4. Connect the 2 quick-release fittings.
5. Attach the engine management wiring harness to the intake manifold.

• | Connect the wiring trough (2).

• | Clip the wiring harness (1) into the guide.

6. Install the ignition module.

Important: When installing a new DIS ignition module, it is not necessary to replace the gaskets.

7. Replace the gaskets (2).
8. Using the KM-6009 (1), install the DIS ignition module.
9. Install the 2 bolts.

Tighten
Tighten the bolts to 8 N·m (71 lb in).

10. Fit the DIS ignition module cover.
11. Connect the DIS ignition module wiring harness plug (2).
12. Clip the engine wiring trough (1) to the cylinder head.