For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery.
2. Remove the instrument panel (I/P) trim panel. Refer to Instrument Panel Trim Panel Replacement .
3. Remove the front floor console. Refer to Front Floor Console Replacement .
4. Remove the I/P padding wiring harness (LAD).
5. Remove the I/P padding wiring harness (RHD).

### Installation Procedure

1. Install the I/P padding wiring harness.
2. Install the I/P trim panel. Refer to Instrument Panel Trim Panel Replacement .
3. Install the front floor console. Refer to Front Floor Console Replacement .
4. Connect the battery.
5. For reprogramming procedures, refer to Control Module References .