For 1990-2009 cars

### Removal Procedure

1. Remove wind protection weatherstrip (1).
2. Remove windshield wiper arms (2).

2.1. | Remove the 2 cover caps.

2.2. | Remove the 2 nuts.

2.3. | Remove the 2 washers.

2.4. | Pull the 2 windshield wiper arms from the shaft.

Important: From the inside, carefully unlatch the clips from the upper bulkhead mounting.

3. Detach the air inlet screen (1).

3.1. | Lever off the air inlet screen in the dash area.

3.2. | Release the 5 clips (3).

3.3. | Detach the windshield washer hose (2).

### Installation Procedure

1. Install the air inlet screen.

1.1. | Attach the windshield washer hose.

1.2. | Install the 5 clips.

Notice: Refer to Fastener Notice in the Preface section.

Important: Make sure the windshield wiper arms are installed in the correct position.

2. Install the windshield wiper arms.

2.1. | Connect the 2 windshield wiper arms to the shafts.

2.2. | Install the 2 washers.

Tighten
Tighten the 2 nuts to 17 N·m (13 lb ft).

2.3. | Install the 2 cover caps.

3. Install the wind protection weatherstrip.