For 1990-2009 cars

### Removal Procedure

1. Remove the complete exhaust system. Refer to Exhaust System Replacement.
2. Remove the front exhaust heat shield.

Loosen the 7 nuts (arrows).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the front exhaust heat shield.

Tighten
Tighten the 7 nuts to 6 N·m (53 lb in).

2. Install the complete exhaust system. Refer to Exhaust System Replacement.