For 1990-2009 cars

### Removal Procedure

1. Remove the roof panel joint finish molding.

1.1. | Remove the roof panel finish molding carefully upwards.

1.2. | Release the 4 clips.

2. Remove the carrier cover for roof luggage carrier fastening holes.

Release the 3 clips (arrows).

3. Remove the roof panel joint finish molding from the bracket.

### Installation Procedure

1. Install the roof panel joint finish molding.

Insert into bracket.

2. Install the roof panel joint finish molding for roof luggage carrier fastening holes.

Install the 3 clips.

3. Install the roof panel joint finish molding.

Install the 4 clips.