For 1990-2009 cars

### Removal Procedure

1. Remove the assist handle.

• | Open the access panel (arrow).

• | Remove the 2 bolts.

2. Remove the clothes hook (1).

Remove the clothes hook connection pin (2).

### Installation Procedure

1. Install the clothes hook.
2. Insert the clothes hook connection pin.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the assist handle.

Tighten
Tighten the 2 bolts to 2.8 N·m (23 lb in).

4. Close the access panel.