For 1990-2009 cars

### Removal Procedure

Warning: Refer to Halogen Bulb Warning in the Preface section.

Remove the bulb.

• | Unscrew the cover (1) in the direction of the arrow.

• | Release the retaining spring (2)

• | Remove the bulb

• | Disconnect the wiring harness plug (3).

### Installation Procedure

Install the bulb.

• | Connect the wiring harness plug.

• | Insert the bulb.

• | Lock the retaining spring.

• | Screw in the cover.