For 1990-2009 cars

### Removal Procedure

1. Remove the control valve body cover. Refer to Control Valve Body Cover Replacement.
2. Remove the shift solenoid valve assembly bolt (315) and the 1 - 2/3 - 4 shift solenoid valve assembly (316).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the 1 - 2/3 - 4 shift solenoid valve assembly (316) and the shift solenoid valve assembly bolt (315)

Tighten
Tighten the bolt to 5.9-7.4 N·m (53-66 lb in).

2. Install the control valve body cover. Refer to Control Valve Body Cover Replacement .