For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat back center cushion cover. Refer to Rear Seat Back Center Cushion Cover Replacement .
2. Remove the lock, rear seat backrest.

• | Remove the upholstery.

• | Unscrew the 2 bolts (1).

3. Replace the frame.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the lock, rear seat back cushion.

Tighten
Tighten the 2 bolts to 42 N·m (32 lb ft).

2. Insert the upholstery.
3. Install the rear seat back center cushion cover. Refer to Rear Seat Back Center Cushion Cover Replacement .