For 1990-2009 cars

### Removal Procedure

Warning: Refer to SIR Inflator Module Handling and Storage Warning in the Preface section.

Warning: Refer to Battery Disconnect Warning in the Preface section.

Warning: Following the deployment of a side impact air bag, inspect the following parts for damage. Replace these parts if necessary:

• | The seat cushion frame

• | The seat recliner, if equipped

• | The seat adjuster

• | The seat back frame

Failure to do so may cause future personal injury.
1. Disconnect the battery.
2. Wait 1 minute for the airbag to deactivate.
3. Remove the front seat belt trim panel (1).
4. Remove the seat belt from the front seat.

Remove the bolt (2).

5. Position the seat in the most forward position.
6. Remove the rear driver seat.

Remove the 2 bolts (1).

Note: Disconnect the wiring harness plug.

7. Remove the front seat.

Remove from the front guide.

8. Partially remove the front seat backrest paneling.

• | Remove the paneling all round (I).

• | Release the 2 clamps (II).

9. Remove the side airbag.

Remove the 3 bolts (1).

10. Remove the side airbag.

Release and disconnect the wiring harness plug.

### Installation Procedure

Note: Ensure the correct wiring harness routing.

1. Install the side airbag.

Connect and latch the wiring harness plug.

Caution: Refer to Fastener Caution in the Preface section.

2. Fasten the side airbag.

Tighten
Tighten the 3 bolts to 5 N·m (44 lb in).

3. Fasten the front seat backrest paneling.

• | Install the 2 clamps.

• | Fasten the paneling all round.

Note: Connect the wiring harness plug.

4. Install the front seat.

Insert into the front guide.

5. Install the rear front seat.

Tighten
Tighten 2 bolts 35 N·m (26 lb ft).

6. Reposition the seat to its original position.
7. Install the seat belt at the front seat.

Tighten
Tighten the bolt 20 N·m (15 lb in).

8. Install the seat belt trim panel.
9. Connect the battery.
10. For programming procedures, refer to Control Module References.