For 1990-2009 cars

## Rear Compartment Floor Panel Carpet Replacement Sedan

### Removal Procedure

1. Remove the rear seat backs.
2. Remove the rear compartment floor carpeting.

### Installation Procedure

1. Position the rear compartment floor carpet into the vehicle.
2. Position the carpet behind the lowered rear seat backs.
3. Raise the rear seat backs.

## Rear Compartment Floor Panel Carpet Replacement Side Wagon

### Removal Procedure

1. Remove the cargo shade.
2. Lower the rear seat back assembly.
3. Gently pull at the attaching clip locations and remove the cargo shade side molding.
4. Remove the seat side bolster.
5. Remove the rear load floor.
6. Remove the cargo net fasteners.
7. Gently pull at the clip locations and remove the rear cargo area side carpet.

### Installation Procedure

1. Install the rear cargo area side carpet to the vehicle with the integral clips making sure that the carpet is slid under the liftgate lower molding.

Notice: Refer to Fastener Notice in the Preface section.

2. Install cargo net fasteners.

Tighten
Tighten the Cargo Net Fasteners to 2.5 N·m (22 lb in).

3. Install the rear seat bolster.
4. Install the rear load floor.
5. Install the cargo shade side molding by pushing at the clip locations.
6. Install the cargo shade.
7. Raise the rear seat back assembly.
8. Install the liftgate weatherstrip over the side carpet using a flat-blade tool.