For 1990-2009 cars

### Removal Procedure

Important: The windshield lower molding locator can only be replaced by removing the windshield and then removing and installing a new windshield moldings, upper, lower locator and both "A" pillar moldings.

1. Remove the windshield. Refer to Windshield Replacement .
2. Remove the lower locator windshield molding from the windshield.
3. Clean the old adhesive from the glass using isopropyl alcohol.

### Installation Procedure

1. Install the windshield lower reveal molding.

Important: Adhesive is already in the service part. No additional adhesive is necessary.

2. Install the windshield. Refer to Windshield Replacement .